**MCH2022 Location Regulations**

**Regarding the use of motorized vehicles\***

**General**

* Normal Dutch traffic regulation apply, unless differently stated here.
* If the vehicle has a seat belt it MUST be worn.
* The holding of communication devices while operating a vehicle is prohibited.
* Maximum speed is 15km/h.
* Maximum speed near people is 5 km/h (walking speed).
* Vehicles may not carry more people than it is designed for (so no people hanging of the vehicle or riding along in the trailer; we have ample bikes available!).
* Vehicles may not be operated by people not licensed or officially trained to do so.
* Reflective clothing has to be worn at all time.
* In case of malfunction or problems; shutdown the vehicle, mark it as out of use and notify management immediately. DO NOT try to fix things yourself!

**Forklift** (including telehandlers with forks)

* The seatbelt has to be worn at any time.
* No lifting of people in any circumstances!
* Approved safety shoes have to be worn.
* Driving with an elevated load is prohibited.
* Within a crowded area the use of a spotter is required. Spotter should wear safety shoes and a helmet.
* Take care of the field. Do not turn the wheels on the spot.

**Boom lift** (including rotating telehandler with platform)

* Harness has to be worn before entering the platform and directly connected.
* Approved safety shoes have to be worn.
* A helmet has to be worn when near the boom lift or on the platform.
* No driving when extended. Only drive with the boom down, and the jib lifted.
* Assign ground support that knows how to get you down in case of trouble. Make sure you have a way of communication (portable radio).
* Use sufficient jack or dirt plates and use stabilizers when available.

**Crane** (Rotating telehandler with winch)

* Direct surroundings should be cleared and sufficient spotters used.
* Spotters and operator should wear safety shoes and a helmet.
* Use stabilizers with sufficient jack plates.

Version 1.0; Manduca

\*) These include, but are not limited to, site carriers, forklift trucks, telehandlers and boom lifts